**STACKED ELECTRIC CONVECTION STEAMERS SPECIFICATIONS**

Stacked Electric Boiler Free Convection Steamers - Shall be model **(2)E-SBC** as manufactured by **Blodgett Oven Corporation**. Convection Steamers shall have all standard features and the following:

**CONSTRUCTION**

* Stainless steel construction
* Stainless steel doors with strong continuous hinge and are field

reversible for left or right swing

* Insulated doors have a one piece, replaceable seal
* Easy open handle and latch provide positive lock and seal when the door

is pushed or slammed shut

* Hidden magnetic door switch cuts power to blower and steam flow to that

cavity, when the door is opened

* Pan support racks shall be polished stainless steel and removable for

easy cleaning

* Electric connectionless steam reservoir is easy to clean through the cavity

door.

**OPERATION**

* ON-OFF rocker switch
* Electronic timer with continuous steam setting
* Timed steam and stop buttons
* Ready light indicates when cavity is ready for steaming
* Unit shall come ready to steam in 15 - 20 minutes from a cold start, and

provide warm cavity-instant steam capacity. Cavity is kept warm and

ready for instant steam between loads.

* Each steamer cavity shall have a powerful side mounted blower, which

increases steam velocity and provides efficient steam distribution

throughout cavity and between loaded pans and no side vents for

increased water/spray resistance.

* Electric-heated steam generating reservoir provides atmospheric steam

to the cavity at approximately 212F. The high-efficiency steam generating

reservoir shall have water level sensors.

* Steam reservoir does not require a pressure gauge or switches
* Automatic drain in steam reservoir

**STANDARD FEATURES**

* Stainless steel stand
* One year parts and labor warranty\*

*\* For all international markets, contact your local distributor.*

**BIDDER REQUIREMENTS:**

* ELIGIBLE BIDDER MUST VISIT JOB SITE.
* ALTERNATES NEED TO BE SUBMITTED FOR APPROVAL 10 DAYS PRIOR TO BID OPENING.
* SUCCESSFUL BIDDER TO DELIVER, UNCRATE, SET IN PLACE, LEVEL, AND REMOVE CRATING.
* FINAL CONNECTIONS BY OTHERS
* BIDDER WILL HONOR PRICES FOR A PERIOD OF ONE YEAR FROM THE BID DATE\_\_\_\_YES\_\_\_\_NO
* BIDDER WILL HONOR PRICING FOR COOPERATIVE PRICING\_\_\_\_YES\_\_\_\_NO

 (Additional travel/mileage charges may apply to systems that are located outside the

 bidding system’s)