**1/3 HP FOOD PROCESSOR**

**Food Processor** - Shall be model FP100 as manufactured by **Hobart**. Food Processor shall have all standard features and the following:

SPECIFICATIONS

* Compact, conveniently designed at 50° angle for operator convenience.
* Small base - occupies minimal counter space.
* Carrying handle on back of housing designed for ease of moving unit.
* Housing constructed of anodized aluminum with rubber feet on base to prevent movement or skidding.
* Removable feed hopper is burnished aluminum.
* Feed hopper, pusher and deflector plate of acetal thermoplastic.
* ELECTRICAL: 120/60/1, 3 Conductor power cord (18 AWG) is 6 feet in length.
* MOTOR: 3.5 amps. Planetary gear driven operating at 420 RPM output, 1⁄3 H.P. with overload protection.
* SWITCHES: Easy to operate (red) OFF and (green)ON switch. Pusher plate and feed hopper interlocks.
* STANDARD EQUIPMENT: Basic unit with deflector plate and cleaning brush.
* WARRANTY: Unit has full one-year warranty on parts, labor and mileage against manufacturer’s defects. Service contracts are available.
* CUTTING TOOLS: Slicer, julienne and dicer plates feature cast aluminum plates with cutlery-grade stainless steel knives. Shredder and grater plates feature stainless steel cutting plates with acetal thermoplastic support hubs.

ACCESSORIES

* 3-Pack Plates: 1⁄16, 5⁄32 slicer plates, 3⁄16 shredder plate, 1 wall rack
* 6-Pack Plates: 1⁄16, 5⁄32, 3⁄8, 7⁄32 slicer plates, 3⁄16 shredder plate and 3⁄8 dicer plate, 2 wall racks
* 3-Peg Wall Rack: designed to hold three plates for additional plate storage
* Slicer Plates: 1⁄16, 5⁄32, 7⁄32, 3⁄8, 5⁄8\* and 3⁄8 HD, 1⁄2, 3⁄16 crimping plate; soft dice 5⁄16, 3⁄8, 1⁄2, 5⁄8
* Julienne Plates: 3⁄32, 3⁄16, 5⁄16
* Dicer Grids: 9⁄32, 3⁄8, 1⁄2, 5⁄8, 3⁄4\*; soft dice 5⁄16, 3⁄8, 1⁄2, 5⁄8

\*NOTE: When you use 5⁄8 slicing plate for dicing, only a DICE-3/4 or 15DICE-5/8L dicer plate can be used.

* Shredder Plates: 1⁄16, 3⁄32, 1⁄8, 3⁄16, 5⁄16, 7⁄32
* Grater Plate: Fine, Extra Fine
* Machine Table: Adjustable height to hold Food Processor
* Adjustable height stainless steel lug cart
* Stainless steel receiving pan
* Plastic receiving pan

**BIDDER REQUIREMENTS:**

* ELIGIBLE BIDDER MUST VISIT JOB SITE.
* ALTERNATES NEED TO BE SUBMITTED FOR APPROVAL 10 DAYS PRIOR TO BID OPENING.
* SUCCESSFUL BIDDER TO DELIVER, UNCRATE, SET IN PLACE, LEVEL, AND REMOVE CRATING.
* FINAL CONNECTIONS BY OTHERS
* BIDDER WILL HONOR PRICES FOR A PERIOD OF ONE YEAR FROM THE BID DATE\_\_\_\_YES\_\_\_\_NO
* BIDDER WILL HONOR PRICING FOR COOPERATIVE PRICING\_\_\_\_YES\_\_\_\_NO

(Additional travel/mileage charges may apply to systems that are located outside the

bidding system’s)