**GAS FLOOR BRAISING PAN SPECIFICATIONS**

GAS FLOOR MODEL BRAISING PAN WITH MANUAL TILT - Shall be model **G-BLT** as manufactured by **Blodgett Oven Corporation**. Braising Pan shall have all standard features and the following:

**CONSTRUCTION**

* 304 stainless steel
* Pan is heavy duty, 10” deep, one piece welded construction
* 5/8” thick stainless steel cooking surface prevents warping or distortion
* Specially designed welded heat transfer fins are heated by the gas

burner/combustion chamber. This combination delivers more uniform

heat transfer over the entire cooking surface.

* Control and tilt mechanism are mounted in stainless steel housings on

the pan body sides

* 100 grit interior finish is coarse enough to retain butter, shortening or

oil during the cooking process, minimizing food sticking and burning

* A heavy-gauge, fully adjustable one-piece cover is standard with torsion

bar type counterbalance designed to maintain selected cover position.

* True rounded leg tubular stand design and 3” radius pan interiors make

cleaning easier.

**OPERATION**

* Electronic intermittent pilot ignition system
* Smooth-action, quick-tilting body with manual crank tilt mechanism, which provides precise control during pouring of pan contents for easy operation
* Pan tilts past vertical for easy cleaning
* Controls allow operation at a 7 degree angle to facilitate griddling.
* Thermostatically controlled for automatic shut-off when desired temperature is reached or heating when temperature falls below desired setting
* High limit thermostat for safety
* Console mounted power switch with indicator light
* Control includes a heat indicator light and temperature control switch
* A vent in the cover top regulates condensate buildup and a rear condensate drip shield is located under the cover to prevent condensate from dripping on floor when cover is opened.

**STANDARD FEATURES**

* Mounting bracket for either right, left or rear faucet mounting
* Etched markings (specify)
  + Gallons
  + Litres
* One year parts and labor warranty\*

*\*For all international markets, contact your local distributor.*

**BIDDER REQUIREMENTS:**

* ELIGIBLE BIDDER MUST VISIT JOB SITE.
* ALTERNATES NEED TO BE SUBMITTED FOR APPROVAL 10 DAYS PRIOR TO BID OPENING.
* SUCCESSFUL BIDDER TO DELIVER, UNCRATE, SET IN PLACE, LEVEL, AND REMOVE CRATING.
* FINAL CONNECTIONS BY OTHERS
* BIDDER WILL HONOR PRICES FOR A PERIOD OF ONE YEAR FROM THE BID DATE\_\_\_\_YES\_\_\_\_NO
* BIDDER WILL HONOR PRICING FOR COOPERATIVE PRICING\_\_\_\_YES\_\_\_\_NO

(Additional travel/mileage charges may apply to systems that are located outside the

bidding system’s)