**HOBART CUTTER MIXER SPECIFICATIONS**

HOBART CUTTER MIXER 450- Shall be model HCM450as manufactured by **Hobart Corporation**. Food Cutter shall have all standard features and the following:

**MODEL**

❑ HCM450 — 45-Quart Cutter Mixer with Stainless Steel Bowl, Stainless Steel Mixing Baffle, Cut/Mix Knife, Knead/Mix Attachment and 6' Power Cable with Plug and Receptacle

❑ HCM450C — Standard 45-Quart Cutter Mixer with Maximum Security Correctional Package (200/60/3 and 460/60/3 only)

**STANDARD FEATURES**

* 5 H.P. Motor
* 45-Quart Capacity Stainless Steel Bowl with Pouring Lip
* Durable Steel Base with Epoxy Enamel Finish
* Electromechanical Safety Interlocks
* Start/Stop Push Button Switches
* 5 Minute Timer with “Hold” and “Jog” Settings
* Counterbalanced Clear Lexan® Polycarbonate Bowl Cover with Stainless Steel Support Bar
* Bowl Tilt Lever
* Stainless Steel Mixing Baffle with Pour-Through Center Shaft
* 2 Blade Cut/Mix Knife
* Knead/Mix Attachment
* Polypropylene Strainer Basket
* 6' Power Cable, Plug and Receptacle

**OPTIONS**

❑ #12 Attachment Hub – Model 84145-1

**ACCESSORIES**

❑ Casters

❑ Extra Basket Kit

❑ 4 Blade Knife

**BIDDER REQUIREMENTS:**

* ELIGIBLE BIDDER MUST VISIT JOB SITE.
* ALTERNATES NEED TO BE SUBMITTED FOR APPROVAL 10 DAYS PRIOR TO BID OPENING.
* SUCCESSFUL BIDDER TO DELIVER, UNCRATE, SET IN PLACE, LEVEL, AND REMOVE CRATING.
* FINAL CONNECTIONS BY OTHERS
* BIDDER WILL HONOR PRICES FOR A PERIOD OF ONE YEAR FROM THE BID DATE\_\_\_\_YES\_\_\_\_NO
* BIDDER WILL HONOR PRICING FOR COOPERATIVE PRICING\_\_\_\_YES\_\_\_\_NO

(Additional travel/mileage charges may apply to systems that are located outside the

bidding system’s)