**Hobart HS7/HS7N Slicer SPECIFICATIONS**

Hobart HS Series Slicer- Shall be Model **HS7/HS7N** as manufactured by Hobart Corporation. Slicer shall have all standard features of HS Series Slicer and the following:

**STANDARD FEATURES**

**KNIFE**

* 13" CleanCut™ Knife
* Removable Ring Guard Cover
* Zero Knife Exposure
* Heavy-Gauge Stainless Steel Knife Cover
* Top-Mounted Borazon Stone Sharpener

**OPERATION**

* 1⁄2 H.P. Knife Drive Motor
* Timing Belt for Automatic Drive System
* Variable Four-Speed Automatic Carriage with Front Mounted Controls
* Three Stroke Lengths

**INTERLOCKS**

* Home-Start Position
* No-Volt Release

**HOUSING AND BASE**

* Burnished Aluminum Base
* Machined Grooves on Gauge Plate and Knife Cover
* Exclusive Tilting, Removable Carriage System
* Electroless Nickel Plated Single Slide Rod with Reservoir Wick in Transport
* Double-Action Indexing Cam
* Ergonomic-Style Handle
* Rear-Mounted, Removable Meat/Vegetable Grip Arm

**OPTIONAL ACCESSORIES / MODIFICATIONS**

* Low Fence
* Food Chute
* Slaw Tray
* Debris Deflector

**BIDDER REQUIREMENTS**

* ELIGIBLE BIDDER MUST VISIT JOB SITE.
* ALTERNATES NEED TO BE SUBMITTED FOR APPROVAL 10 DAYS PRIOR TO BID OPENING.
* SUCCESSFUL BIDDER TO DELIVER, UNCRATE, SET IN PLACE, LEVEL, AND REMOVE CRATING.
* FINAL CONNECTIONS BY OTHERS
* BIDDER WILL HONOR PRICES FOR A PERIOD OF ONE YEAR FROM THE BID DATE\_\_\_\_YES\_\_\_\_NO.
* BIDDER WILL HONOR PRICING FOR COOPERATIVE PRICING\_\_\_\_YES\_\_\_\_NO.

(Additional travel/mileage charges may apply to systems that are located outside the bidding system’s area)